HIGH POWER PoE INJECTOR (PS-POE-AT-TC)

1) 용  도

본 기기는 고전력 PoE 인젝터로, 한 가닥의 카테고리 케이블에 전력과 데이터를 동시에 공급할 수 있도록 전원을 공급해주는 기기이며 최대 100미터의 전송을 지원한다.

2) 기  능

- 10/100/1000 (MbPS) 데이타 전송률 지원

- IEEE802.3af 규격 충족

- 부하 측정 LED

- 100/240 VAC 유니버셜 전원 입력 지원

3) 사  양

- DIMENSIONS (HWD): 5 1/2" x 2 1/8" x 1 1/4" (14 cm x 5.3 cm x 3.25 cm)

- WEIGHT: .44 lbs (200 g)

ENVIRONMENTAL

- Temperature (Operating):

-4°F to 104°F (-20°C to 40°C) @ 30W,

-4°F to 131°F (-20°C to 55°C) @ 22.5W

- Temperature (Storage): -4°F to +158°F (-20°C to +70°C)

- Relative Humidity (Operating): Maximum 90%, Non-Condensing

- Thermal Rating: 20 BTU/hr (@240VAC)

- Operating Altitude: -1000 to 10,000 ft. (-304.8 to 3048 m)

GENERAL

L- EDs:

Yellow (On): power is on and active

Green (On): A remote terminal is connected

Green (Blinking): Overload state or short circuit

- Enclosure: Molded black matte plastic

- Cord and Connectors: Dual shielded RJ45 jacks built into the enclosure, EIA 568A and 568B

- Approvals:

IEEE 802.3at (PoE)

RoHS / WEEE compliant

CE

FCC Part 15, Class B

EN 55022 Class B (Emissions)

EN 55024 (Immunity)

VCCI (Japan)

C-Tick

UL/cUL per IEC 60950-1

GS Mark per IEC 60950-1

INPUT SPECIFICATIONS

- AC Input Voltage Range: 100-240 VAC

- AC Input Current: 0.8A @ 100-240 VAC

- AC Frequency: 50 to 60 Hz

- AC Input Current: 0.8A MAX at 110-240 VAC

- Protection: Internal Primary Current Fuse, Inrush Limiting

- Input Power Cord: Universal Power Cord, 3 Foot

OUTPUT SPECIFICATIONS

- Pass Through Data Rates: 10/100/1000 Mbps

- Output Voltage: 55 VDC Nominal

- Output Power: 30 Watts (Guaranteed)

- Output Current: 0.6A (max)

- Ripple and Noise: Below the IEEE802.3af requirements

- f<500Hz: Vp-p 0.5

- 500Hz to 150kKHz: Vp-p 0.2

- 150KHz to 500KHz: Vp-p 0.15

- 500KHz to 1MHz: Vp-p 0.1

- Transient Response: Meets IEC61000-4-4 (1Kv)

- DXLink Transport Layer Throughput: 10.2 Gbps pass thru (only applicable to DXLink signals)