SINGLE MODE FIBER OUTPUT BOARD (DGX-O-DXF-SMS)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 멀티모드 옵티컬 출력 보드이며, 4개의 광출력 SFP 모듈이 지원되며 멀티모드 광 출력은 300m 까지 오디오, 비디오 신호 전송을 지원한다.

2) 기  능

- HDCP 준수 비디오 신호 광 전송

- 10Gbps 전송 대역폭

- 광 출력을 통한 독립적인 신호전송과 안정성 확보

- SFP 모듈 사용으로 간편한 교체 가능

3) 사  양

GENERAL

- Compatible AMX Products: Must be used in conjunction with an Enova DGX 8, 16, 32 or 64 Digital Media Enclosure and a DXLink HDMI Single Mode Fiber Receiver, Duplex (FG1010-560)

- Regulatory Compliance: See Enova DGX Digital Media Switcher Enclosure for regulatory compliance

- Safety Certification: Class 1 Eye safe per requirements of IEC 60825-1 / CDRH

- Recommended Accessories: DXLF-HDMIRX-SM-D, DXLink HDMI SM Fiber RX, Duplex (FG1010-560)

SIGNAL TRANSPORT – DXLINK W/ SINGLE MODE FIBER, DUPLEX

- Compatible Formats: HDMI Video / Audio / Ethernet / USB (HID) Keyboard & Mouse /Control

- Signal Type Support: DXLink Single Mode Fiber, Duplex

- Connectors: (4) Duplex LC Fiber Ports, conforming to ANSI TIA/EIA 604-10 (FOCIS 10A)

- Transport Layer Throughput (Max): 10.3125 Gbps

- Fiber Transceiver Type: 10G SFP+

- Fiber Cable Type: 9/125µm

- Fiber Cable Length: Up to 10 km (6.21 miles)

- Optical Wavelength: 1310 nm

- Single Mode Optical Budget: 7.4 dB (typ), 5.1 dB (stressed) between DXLink Fiber Transceivers

- Optical Modulation Amplitude (OMA): -5.2 dBm (min)

- Optical Modulation Amplitude (OMA) Sensitivity: -12.6 dBm (typ), -10.3 dBm (stressed)

- Single Mode Optical Transceiver Mean Output Power: -8.2 dBm to 0.5 dBm (average power)

- DXLink Fiber Output Board Propagation Delay: 5 us

- Video Data Rate (Max):

4.95 Gbps / 5.568 Gbps

5.568 Gbps supported when the HDMI Output Board scaler or DXLink RX scaler is in Bypass mode using CEA-861 formats and resolution is 1080p60 or less

- Video Pixel Clock (Max):

165 MHz / 185.625 MHz

185.625 MHz supported when the HDMI Output Board scaler or DXLink RX scaler is in Bypass mode using CEA-861 formats and resolution is 1080p60 or less

- Progressive Resolution Support: 480p up to 1920x1200 @ 60 Hz

- Interlaced Resolution Support: 480i, 576i, 1080i

- Deep Color Support:

24-bit, 30-bit

30-bit supported when the HDMI Output Board Scaler or DXLink RX Scaler is in Bypass mode and format is 1080p60 or less

- Color Space Support: RGB 4:4:4, YCbCr 4:4:4 and 4:2:2

- Input signal support for YCbCr: 4:4:4 and 4:2:2, output color-space is converted to RGB 4:4:4

- 3D Format Support

Yes (scaler on corresponding output board or RX must be set to bypass mode)

Frame Packing 1080p up to 24 Hz

Frame Packing 720p up to 50/60 Hz

Frame Packing 1080i up to 50/60 Hz

Top-Bottom 1080p up to 24 Hz

Top-Bottom 720p up to 50/60 Hz

Side-by-Side Half 1080i up to 50/60 Hz

- Audio Format Support:

Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM

Dolby Digital and DTS support up to 48 kHz, 5.1 channels

- Audio Resolution: 16 bit to 24 bit

- Audio Sample Rate: 32 kHz, 44.1 kHz, 48 kHz, 96 kHz, 192 kHz

- Local Audio Support:

Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel when used in conjunction with Enova DGX Audio Insert / Extract Board

- HDCP Support: Yes, full matrix HDCP support (includes any input to any or all outputs)

- Key Management System:

AMX HDCP InstaGate Pro Technology

Key support up to 16 sinks per output, independent of source device

- CEC Support: None