TWISTED PAIR INPUT BOARD (DGX-I-DXL)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 네트워크 케이블 입력 보드이며, 4개의 RJ45 포트가 오디오, 비디오, 컨트롤, 이더넷, 파워 전송을 지원한다.

2) 기  능

- 한 가닥의 네트워크 케이블로 오디오, 비디오, 컨트롤, 이더넷, 파워 전송

- HDMI 신호를 최대 100m 전송

- 핫스왑 기능

- 3D 비디오 지원

- 서라운드 오디오 지원

- HDCP 준수

3) 사  양

GENERAL

- Compatible AMX Products:

Must be used in conjunction with an Enova DGX 8, 16, 32 or 64 Digital Media Enclosure and a DXLink Twisted Pair Transmitter

Compatible with all AMX DXLink Twisted Pair Transmitters including HDMI Transmitter Module, Multi-Format Decor Style Wallplate and Multi-Format Wallplate

- Recommended Accessories:

AVB-TX-MULTI-DXLINK DXLink Multi-Format Transmitter (FG1010-310)

AVB-DWP-TX-MULTI-DXLINK DXLink Multi-Format Decor Style Wallplate Transmitters (US) (FG1010-325-BL/WH)

AVB-WP-TX-MULTI-DXLINK DXLink Multi-Format Wallplate Transmitters (FG1010-320-BL/WH)

USB (HID) Keyboard & Mouse

- USB (HID):

Use the Enova DGX Digital Media Switcher in conjunction with DXLink Transmitters and Receivers (twisted pair and/or fiber), connect a DXLink Transmitter to a PC and a DXLink Receiver to a keyboard and mouse, the system then emulates commands from the receiver back to the PC.

Signal Transport – DXLink w/HDCP

- Compatible Formats: HDMI Video/Audio/Ethernet/USB (HID) Keyboard & Mouse/Power and Control

- Signal Type Support: DXLink Twisted Pair

- DXLink Twisted Pair Power:

The DXLink Twisted Pair Input Board provides Power over DXLink

DXLink Multi-Format Wallplate Transmitters require a DXLink Power sourcing device, DXLink Transmitter Modules can be powered via DXLink Power or desktop power supply (ENERGY STAR® qualified) with power cord

- Approved Power over DXLink sourcing devices include:

Enova DGX 8/16/32/64 Digital Media Switcher (with a DXLink Twisted Pair Input Board installed)

Compatible Enova DVX All-In-One Presentation Switcher (3155HD, 3156HD or 2155HD)

PS-POE-AT-TC High Power PoE Injector

PDXL-2 Power over DXLink Controller

- Connectors: (4) RJ-45 Ports

- Transport Layer Throughput (Max): 10.2 Gbps

- Twisted Pair Cable Type:

Shielded Cat6, Cat6A and Cat7, DXLink twisted pair cable runs for DXLink equipment shall only be run within a common building where a common building is defined as: the walls of the structure(s) are physically connected and the structure(s) share a single ground reference.

- Twisted Pair Cable Length: Up to 328 ft (100 m)

Video Data Rate (Max):

4.95 Gbps / 6.75 Gbps

6.75 Gbps supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Video Pixel Clock (Max):

165 MHz / 225 MHz

225 MHz supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Progressive Resolution Support: 480p up to 1920x1200 @ 60 Hz

- Interlaced Resolution Support: 480i, 576i, 1080i

- Deep Color Support:

24-bit, 30-bit, 36-bit

30-bit, 36-bit supported when the HDMI Output Board Scaler or DXLink HDMI RX Scaler is in Bypass mode and format is 1080p60 or less

- Color Space Support:

RGB 4:4:4

YCbCr 4:4:4 and 4:2:2

Input signal support for YCbCr 4:4:4 and 4:2:2, output color-space is converted to RGB 4:4:4

- 3D Format Support:

Yes (HDMI Primary Formats, when used with DXLink Output Boards and the DXLink HDMI RX Scaler is in bypass mode)

Frame Packing 1080p up to 24 Hz

Frame Packing 720p up to 50/60 Hz

Frame Packing 1080i up to 50/60 Hz

Top-Bottom 1080p up to 24 Hz

Top-Bottom 720p up to 50/60 Hz

Side-by-Side Half 1080i up to 50/60 Hz

- Audio Format Support:

Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM

Dolby Digital and DTS support up to 48 kHz, 5.1 channels

- Audio Resolution: 16 bit to 24 bit

- Audio Sample Rate: 32 kHz, 44.1 kHz, 48 kHz, 96 kHz, 192 kHz

- Local Audio Support:

Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel when used in conjunction with Enova DGX Audio Insert / Extract Board

- HDCP Support:

Yes, full matrix HDCP support (includes any input to any or all outputs)

Key Management System

- AMX HDCP InstaGate Pro Technology:

Key support up to 16 devices per output, independent of source device

- CEC Support: None

- ICSP, TCP/IP, USB, IR, Control Management:

Control distribution is managed by the Enova DGX 8/16/32/64 Digital Media Switcher on-board NetLinx Master and Ethernet Switch

- DDC/EDID Support:

EDID provided by the Enova DGX 8/16/32/64 Digital Media Switcher to the connected DXLink HDMI TX, EDID is user re-programmable

- DXLink Input Board Propagation Delay: 5 us