TWISTED PAIR 4K INPUT BOARD (DGX-I-DXL-4K)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 4K UHD 해상도를 지원하는 네트워크 케이블 입력 보드이며, 4개의 RJ45 포트가 오디오, 비디오, 컨트롤, 이더넷, 파워 전송을 지원한다.

2) 기  능

- 4K UHD 해상도 지원

- 한 가닥의 네트워크 케이블로 오디오, 비디오, 컨트롤, 이더넷, 파워 전송

- HDMI 신호를 최대 100m 전송

- 핫스왑 기능

- 3D 비디오 지원

- 서라운드 오디오 지원

- HDCP 준수

3) 사  양

- Compatible Formats: HDMI Video, Audio, Ethernet, USB (HID), Power, Serial Control and IR Control

- Signal Type Support: DXLink Twisted Pair

- Connectors: (4) RJ-45 Ports

- Progressive Resolution Support:

480p up to 4096 x 2160p, 60 Hz* (*Y/Cb/Cr 4:2:0, with 4K RX Scaler in Bypass mode)

- Interlaced Resolution Support: 480i, 576i, 1080i

If input is interlaced, all scaled outputs will deinterlace video to a progressive resolution format. If in scaler Bypass mode, interlaced input will pass through unaltered.

4K Resolution Support:

3840 x 2160p @ 24/25/30 Hz

4096 x 2160p @ 24/25/30 Hz

3840 x 2160p @ 60 Hz, 4:2:0*

4096 x 2160p @ 60 Hz, 4:2:0*

Supported by DX-RX-4K when in Bypass Scaling mode

- Audio Format Support:

Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM (Dolby Digital and DTS support up to 48 kHz, 5.1 channels)

- Compatible AMX Products:

Must be used in conjunction with an Enova DGX 800, 1600, 3200 or 6400 Digital Media Enclosure and a DXLink Twisted Pair Transmitter.

Compatible with all AMX 4K DXLink Twisted Pair Transmitters including 4K HDMI Decor Style Wallplate, 4K Solecis Digital Switchers (including 4x1, 5x1 and 8x1). Also compatible with (non 4K) DXLink Twisted Pair Transmitters including HDMI Transmitter Module, Multi-Format Decor Style Wallplate, and Multi-Format Wallplate, and Solecis Digital Switchers (including 4x1, 5x1 and 8x1).

For passage of 4K signal content, DXLink Twisted Pair 4K Boards must be used in conjunction with DXLink Twisted Pair 4K Transmitters and Receivers.