DVI INPUT BOARD (DGX-I-DVI)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 DVI 케이블 입력 보드이며, 4개의 DVI 포트가 HDMI, DISPLAYPORT++, DVI 신호를 지원한다.

2) 기  능

- InstaGate Pro® HDCP 인증키 기술

- 핫스왑 기능

3) 사  양

DVI w/HDCP

- Compatible Formats: DVI, HDCP

- Signal Type Support:

DVI-D (Single Link)

HDMI (With DVI Cable Adapter)

DisplayPort ++ (Input Only, With DVI Cable Adapter)

HDMI Mode Support: DVI boards can be run in HDMI mode with an EDID update which will provide full HDMI functionality and board specifications

- Video Data Rate (Max): 4.95 Gbps

- Video Pixel Clock (Max): 165 MHz

- Progressive Resolution Support: 480p up to 1920x1200 @ 60 Hz

- Interlaced Resolution Support: 480i, 576i, 1080i

- 2K Resolution Support:

2048x1024 @ 47 Hz, 2048x1080 @ 60 Hz, 2048x1152 @ 60 Hz, 2048x1536 @ 24 Hz

Note: 2K formats are only compatible with the DVI and HDMI Input/Output boards and require the output scaler to be set in Bypass mode

- Input Equalization:

Adaptive up to 100 ft (30 m) at 165 MHz

Cable distance support dependent on cable type and signal format

- Input Re-clocking (CDR): Yes

- Color Depth Support: 24-bit

- Color Space Support: RGB 4:4:4

- Local Audio Support: Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel

- DDC/EDID Support:

EDID provided by Enova DGX 8/ 16 / 32 / 64

EDID is user re-programmable

- HDCP Support: Yes, full matrix HDCP support (includes any input to any or all outputs)

Key Management System

- AMX HDCP InstaGate Pro Technology:

Key support up to 16 devices per output, independent of source device

- Input Voltage (Nominal): 1.0 Vpp Differential

- DVI Input Board Propagation Delay: 2 us

HDMI Audio Synchronization (relevant to DVI when DVI board is used in HDMI mode): Progressive and Interlaced Video Formats @ 60 Hz frame rate: Audio is actively delayed to match video within 8ms leading or lagging.

- Connectors: 4 DVI-I Ports (DVI-D Single Link is the supported signal type)