AUDIO SWITCHING BOARD KIT FOR ENOVA DGX 800/1600 (DGX800/1600-ASB)

1) 용  도

본 기기는 Enova DGX 800/1600 전용 오디오 스위칭 보드로서 입/출력 보드 페어로 구성되어 있다. 카드를 장착하면 오디오 스위칭 기능을 사용할 수 있다. 오디오 DSP 내장으로 10밴드 파라메트릭 이퀄라이저가 각각의 출력에 제공되며 웹 인터페이스를 통해 간편하고 손쉬운 설정 및 모니터링을 제공한다.

2) 기  능

- 16x16 (DGX 800), 24x24 (DGX 1600) 오디오 스위칭

- 오디오 DSP 내장

3) 사  양

- COMPATIBLE ENOVA DGX SYSTEMS: Enova DGX 800, Enova DGX 1600

- COMPATIBLE ENOVA DGX I/O BOARDS:

DGX-I-HDMI-4K, Enova DGX 4K HDMI Input Board (FG1061-540)

DGX-I-HDMI, Enova DGX HDMI Input Board (FG1058-540)

DGX-O-HDMI, Enova DGX HDMI Output Board (FG1058-550)

DGX-I-DVI, Enova DGX DVI Input Board (FG1058-600)

DGX-O-DVI, Enova DGX DVI Output Board (FG1058-610)

DGX-I-DXL-4K, Enova DGX 4K DXLink Twisted Pair Input Board (FG1058-570)

DGX-I-DXL, Enova DGX DXLink Twisted Pair Input Board (FG1058-570)

DGX-O-DXL-4K, Enova DGX 4K DXLink Twisted Pair Output Board (FG1061-580)

DGX-O-DXL, Enova DGX DXLink Twisted Pair Output Board (FG1058-580)

DGX-I-DXF-MMD, Enova DGX DXLink Multimode Fiber Input Board, Duplex (FG1058-622)

DGX-O-DXF-MMD, Enova DGX DXLink Multimode Fiber Output Board, Duplex (FG1058-632)

DGX-I-DXF-MMS, Enova DGX DXLink Multimode Fiber Input Board, Simplex (FG1058-623)

DGX-O-DXF-MMS, Enova DGX DXLink Multimode Fiber Output Board, Simplex (FG1058-633)

DGX-I-DXF-SMD, Enova DGX DXLink Single Mode Fiber Input Board, Duplex (FG1058-620)

DGX-O-DXF-SMD, Enova DGX DXLink Single Mode Fiber Output Board, Duplex (FG1058-630)

DGX-I-DXF-SMS, Enova DGX DXLink Single Mode Fiber Input Board, Simplex (FG1058-621)

DGX-O-DXF-SMS, Enova DGX DXLink Single Mode Fiber Output Board, Simplex (FG1058-631)

- AUDIO SWITCHING:

16x16 (DGX 800) or 24x24 (DGX 1600) Matrix Audio Switching. Each of the embedded or auxiliary analog audio outputs has independent volume, EQ and sync delay

AUDIO INPUTS

- Auxiliary Analog Audio Input Connections:

(4) 3.5 mm 10-position captive-wire terminals; support balanced (differential) or unbalanced (single-ended) stereo audio

8 or 16 Embedded digital audio inputs from video input positions (Embedded audio must originate as 2 channel PCM) - Applies to embedded audio inputs on Enova DGX Input Boards for positions 1-8 (DGX 800) / 1-16 (DGX 1600)

8 Auxiliary audio inputs on the Input Board of the Audio Switching Board Kit - Audio inputs 9-16 (DGX 800), 17-24 (DGX 1600)

AUDIO OUTPUTS

- Auxiliary Analog Audio Output Connections:

(4) 3.5 mm 10-position captive-wire terminals; support balanced (differential) or unbalanced (single-ended) stereo audio

8 or 16 Embedded digital audio to video outputs - Applies to embedded audio outputs on Enova DGX Output Boards for positions 1-8 (DGX 800) / 1-16 (DGX 1600)

8 Auxiliary audio outputs on the Output Board of the Audio Switching Board Kit – Audio outputs 9-16 (DGX 800, 17-24 (DGX 1600)

AUDIO ADJUSTMENTS PER INPUT (EMBEDDED VIDEO AND AUXILIARY INPUTS)

- Audio Input Compression: Independent Compression per input

- Attack: 1 to 2000 ms

- Release: 10 to 5000 ms

- Compression Ratio: 1 to 20

T- hreshold: -60 to 0 dB

- Audio Input Gain Compensation: -24 dB to +24 dB, 1 dB steps

AUDIO ADJUSTMENTS PER OUTPUT (EMBEDDED VIDEO AND AUXILIARY OUTPUTS)

- Audio Output Compression:

10-band parametric EQ with variable center frequency, filter type and Q per band

Center Frequency: 20 Hz to 20 kHz

- EQ Gain: -12 to +12 dB

- Q: 0.1 to 20

- Filter Types: Bell, Base Shelving, Treble Shelving, Low Pass, High Pass, Band Pass, Band Stop

- Audio Output Sync Delay: 0 to 200 ms

- Balance Control: 20 steps each left and right

- Independent EQ, Volume and Balance control per output

- Test Tone Generator:

Single selection of test tone type available on all outputs simultaneously. Individually enabled/disabled per output – 60 Hz, 250 Hz, 400 Hz, 1 kHz, 3,Hz, 5 kHz, 10 kHz, Pink Noise, White Noise

AUXILIARY ANALOG AUDIO INPUTS

- Input Level (Nominal): +4 dBu (1.228 Vrms) balanced or -10 dBV (0.3162 Vrms) unbalanced

- Input Level (Maximum): +14 dBu

- Input Impedance: >17 kOhms balanced, >10 kOhms unbalanced

- Audio Channel Crosstalk:

Balanced Line Inputs: -98 dB @ 0 dBV, 20 Hz to 20 kHz, Unbalanced Line Inputs: -70 dB @0 dBV, 20 Hz to 20 kHz

AUXILIARY ANALOG AUDIO OUTPUTS

- Output Level (Maximum): +17 dBu (line level)

- Output Impedance: 200 Ohms (line level)

- Audio Frequency Response: Line: 20 Hz to 20 KHz +/-0.1 dB

- Audio S/N Ratio: Line: 105 dB @ 10 dBV, AES17

- Audio THD+N: Line: 0.003% @ 0 dBV, 1 kHz

- DOWN-MIX:

Down-mix input fed from selectable embedded audio input from any Enova DGX Input Board. Down-mixed audio switchable to all embedded/auxiliary audio outputs.

Down-mix input format support: Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM