POWER DISTRIBUTOR (SEQ-1216i)

1) 용  도

본 기기는 AV 장비를 보호하는 데 필요한 전력 보장, 과부하 방지 차단, 4그룹 순차전원 On/Off 및 서지 보호 기능을 제공하는 순차 전원 분배기이다. 설치, 프로그램, 운영이 간편하며 다용도 매니지먼트 기능을 가지고 있다. 상시전원 공급되는 2개의 콘센트와 4개의 프로그램 가능한 뱅크가 탑재되어 있다. 원격 장치를 제어하기 위한 하나의 가상 뱅크을 갖추고 있어, 분배 체계를 제한 없이 확장할 수 있다. AV장비의 성능을 저하시키는 혼합접지나 커먼모드 잡음과 같은 부작용을 일으키지 않으면서 최대 6,000V까지 전압이 급등하는 것을 차단한다. 또한 완전한 전원 컨디션 솔루션을 위한 커먼모드 및 노멀모드 Impedance TolerantⓇ EMI/RFI filtering, SurgeX ICEⓇ -Inrush Current Elimination and COUVSⓇ -Catastrophic Over/Under Voltage Shutdown 기능을 제공한다.

2) 기  능

- 자기 차폐 금속 케이스

- 2개의 소켓으로 구성된 4개의 순차전원 뱅크, 2개의 상시전원

- EMI / RFI 필터

- COUVS® 과전압 또는 과소 전압 폐쇄

- SurgeX ICE® 전압 유입 제거

- 최대 6,000V의 서지 에너지 제거

3) 사  양

- Power Configuration : 16 Amps @ 230 volts, 50Hz / 60Hz

- Power Requirement (no load): 15 watts.

- Number Of Sequenced Banks : 4 (2 receptacles each bank)

- Number Of Always On Receptacles : 2

- Surge Let-Through Voltage (6000-volt surge): 0 volts.

- Safety Certification : IEC/EN 61643-1

- Performance Rating: Grade A, Class 1, Mode 1

- Maximum Applied Surge Voltage: 6000 volts

- Undervoltage Shutdown : 180 volts (auto resetting)

- Overvoltage Shutdown : 280 volts (auto resetting)

- Remote Turn-on Applied Voltage Range: 5 to 30 volts DC

- Auxiliary Relay Contact Rating: 30 Volts at 1 Amp

- Delay Time Per Bank : 2,5,10,15,20 sec. (Switchable)

- Dimensions (WxHxD): 483 x 45 x 267 mm

- Weight: 5 kg