WIRELESS MICROPHONE SYSTEM (WMS470 VOCAL SET D5)

1) 용  도

본 기기는 다 채널 무선 마이크 시스템으로서, 자연스러운 사운드를 제공하며 습기 차폐를 통해 마이크에 대한 높은 수준의 습기 보호를 보장한다. 또한 동일한 주파수 대역 내에서 최대 48개 채널로 전송할 수 있으며 안테나 스플리터, 전원 공급 장치 및 안테나를 사용하여 확장된 무선 시스템을 설치 할 수 있다.

2) 기  능

- 자동 주파수 설정

- 최대 16개의 사전 프로그래밍 된 주파수 제공

- 파일럿 톤을 통한 시동 소음을 방지

- 최대 14시간의 배터리 수명 및 배터리 상태 정보

- 2색 디스플레이 백라이트

3) 사  양

- package includes : 1 x SR470 Receiver

: 1 x HT470 Handheld transmitter with D5 capsule

: 1 x Stand adapter

: 1 x Rack mount kit

: 1 x Universal power supply with US/UK/EU adapter

: 1 x AA size battery

: 2 x Antennas

- Model : SR470

- Switching bandwidth : 30.5 MHz

- Diversity System : Microprocessor-controlled diversity

- Modulation : Wideband FM

- Audio bandwidth : 35 – 20000 Hz (± 3 dB)

- T.H.D : <= 0.3 %

- SNR (A-weighted) : typ. 120 dB(A)

- Audio outputs : 1 x XLR sockets balanced

: 1 x TS 1/4” / 6.3 mm jack sockets unbalanced

- Standard Accessories : 2 UHF antennas, power supply, rack mount kit

- Dimension (H x W x D)mm : 44 x 202 x 190

- Weight : 972g

- Model : HT470

- frequency bandwidth : 35 to 20000 Hz

- Signal to Noise : 120 dB-A

- THD at 1 kHz :  0.7 Prozent

- Operating temperature range  : -10 to 55 Celsius

- Peak deviation : 48 kHz

- Switching bandwidth : 30 MHz

- Recommended simultaneous channels : 24

- Radio range (Line of sight) : 100m (depending on antenna system)

- Nominal deviation : 20 kHz

- Radio Output Power (min/max) : 10 to 50 mW

- Battery type : LR6 AA alkaline , HR 6 AA (NiHM) , FR 6 AA lithium

- Finish : black

- Dimension (H x W)mm : 237 x 51

- Weight : 240g