HIGH-PERFORMANCE WIRELESS MICROPHONE SYSTEM (PERCEPTION WIRELESS VOCAL SET)

1) 용  도

본 기기는 무선 마이크 시스템으로서, 최대 8채널을 서로 다른 채널 사전 설정으로 운영할 수 있으며 소규모 클럽, 예배당, 회의실, 기악 및 성악 공연에 사용하기에 적합하다. 또한 시스템 상태를 쉽게 모니터링 할 수 있도록 오디오 클리핑 및 RF 신호 LED를 제공한다.

2) 기  능

- 30MHz 선택 대역폭

- 단일 AA 크기 배터리로 8시간 작동

- 자동 설정 모드

- 전원 스위치 모드

3) 사  양

- package includes : 1 x SR45 Receiver

1 x HT45 Handheld transmitter

1 x Stand adapter

1 x Universal power supply with US
- Model : SR45

- Carrier Frequency Range : 500 - 865 MHz

- Modulation : FM (Frequency Modulation)

- Audio bandwidth : 40 - 20,000 Hz (+/- 3dB)

- T.H.D. at 1 kHz : typ. 0.8%

- Signal/Noise Ratio : typ. 105 dB(A)

- Squelch Threshold : -100 to -70 dBm adjustable

- Audio Outputs : Balanced XLR and unbalanced 1/4" (6.3 mm) jack

-adjustable from mic to line level.

Output level at rated deviation = 500 mV rms

- Dimension (H x W x D)mm : 44 x 190 x 200

- Weight : 360g

- Model : HT45

- Carrier Frequency Range : 500 - 865 MHz

- Modulation : FM

- Nominal Deviation : 15

- RF Output : 10mW

- Polar Pattern : Cardioid

- Microphone Head Versions : P5

- Switching Bandwidth : 30MHz

- Recommended Simultaneous Channels : 5

- Number of Selectable Frequencies : 8 Fixed Frequencies

- Frequency Selection : Fixed Frequency

- Radio Range (Line of sight) : 30m

- Power Requirement : 1x 1.5 V AA size battery

- Battery Rife : 10 hours

- Dimensions : 237 x 51mm

- Weight : 214g