LOUDSPEAKER (VPX715)

1) 용  도

본 기기는 15“ 2-WAY 풀레인지 라우드 스피커로써 라이브 음악 및 스피치를 위한 공간에 적용된다. 70°×60°의 커버리지 패턴으로 균일하고 부드러운 소리를 제공하며 DuraFlex 코팅 마감과 16게이지 스틸 그릴로 인클로저 내부를 보호한다.

2) 기  능

- 15인치 고효율 로우 드라이버

- 70°×60° 커버리지 패턴

- 1.5“ 폴리머 다이어프램 압축 드라이버

- 합판으로 제작, DuraFlex TM 코팅 마감된 인클로저

- 손쉬운 운반을 위한 2개의 일체형 핸들

- 16게이지 스틸로 제작된 그릴

3) 사  양

- Frequency Range (-10 dB) : 47 Hz - 20 kHz

- Frequency Response (±3 dB) : 80 Hz - 20 kHz

- Coverage : 70° × 60° (H × V)

- Crossover Mode : Passive

- Crossover Frequency : 2.0 kHz

- Power Rating : 450 W/900 W/1800 W (Continuous/Program/Peak)

- Sensitivity (1w@1m) : 98 dB

- Nominal Impedance : 8 Ohms

- Maximum SPL : 125 dB (131 dB peak)

- LF Driver : 1 × 15” (381.00 mm) woofer

- HF Driver : 1 × JBL 2408H-2 tweeter

- Enclosure : Trapezoidal, 15/18 mm, plywood

- Suspension / Mounting : 13 points (3@top, 3@bottom, 2@each side, 3@rear),
M10 thread hardware; Dual-angle 35 mm pole socket

- Transport : 2 × die-cast handles with backing cup

- Finish : Black DuraFlexTM finish

- Enclosure Construction : Powder coated, black, 16-gauge perforated steel
with acoustically transparent black screen backing

- Input Connector : 2 × Neutrik® Speakon® NL-4

- Dimensions (H×W×D) : 701 × 432 × 470 mm

- Weight : 25.34 Kg