MAIN LINE-ARRAY SPEAKER

1) 용  도

본 기기는 기업, 극장, 예배당 등의 소/중형 공간의 설치를 위한 컴팩트형 라인어레이 스피커이다. 최신형 트랜스듀서 및 웨이브가이드 기술을 적용하여 고성능과 고효율 및 110도의 일관성 있는 수평 커버리지를 제공한다. 스피커는 2개의 8“ LF 드라이버, 4개의 3.5” MF 드라이버, 2개의 2“ HF 드라이버로 구성되었다. 독점적인 기술인 이중 플레어형 저주파 포트로 주파수 범위를 49Hz까지 확장하며 저주파 성능을 극대화한다. 또한 특허 인증을 취득한 서스펜션 시스템을 통해 편리하게 설치할 수 있으며 다양한 옵션 액세서리가 구성되어있다.

2) 기  능

- Differential Drive ™ 우퍼와 Slip Stream ™ 포트는 49Hz까지 저음 응답 제공

- MF RBI (Radiation Boundary Integrator) 기술로 수평 지향각 향상

- HF 압축 드라이버는 우수한 음질과 일관성을 제공

- 내장형 MF / HF 패시브 네트워크로 앰프 채널 감소

- HiQnet Performance Manager™를 통한 컨트롤

- 다양한 마운팅 액세서리로 설치 옵션 확장

- 자동 잠금 장치 메커니즘으로 간편하고 안전하게 설치

- 내후성을 위한 전면 밀폐형 그릴 커버 (IP55)

- 작고 가벼운 디자인

3) 사  양

- System type : Bi-amp 3-Way system

- Frequency Range (-10dB) : 49Hz ~ 19kHz

- Horizontal Coverage : 110 deg.

- Vertical Coverage : Varies with array size and configuration

- Power rating	: LF 600W Continuous (IEC/100 hour)

: MF/HF 390W Continuous (IEC/100 hour)

- Max SPL : 139 dB

- Impedance : LF 8 ohms, MF/HF 8 ohms

- Transducers : LF 2x8“, MF 4x3.5”, HF 2x2“

- Suspension degree : 0.25, 0.5, 1, 1.5, 2, 2.5, 3, 4, 6, 8, 10

- IP Rating : IP55 (IEC 60529)

- Connectors : Neutrik® SpeakON® NL-4 (2x)

- Dimension (H x W x D)mm : 226.60 x 761.29 x 375.16

- Weight : 29.5 kg