ACTIVE BEAM STEERING POWERED LOUDSPEAKER ARRAY (DC430)

1) 용  도

본 기기는 디지털 신호를 통해 제어하는 파워드 어레이 스피커로 탁월한 음성 명료도를 제공하며 최대 50m까지 일정한 음압 레벨을 제공한다. 17개의 커스텀 디자인 된 4“ 라우드 스피커는 16채널 D-클래스 앰프에 의해 구동되며 특허 받은 알고리즘에 따라 배열된다. 전용 소프트웨어를 통한 빔 조정 매개 변수, 오디오 처리, 사전 설정 및 모니터링에 대한 제어 기능을 제공하며 원하는 색상으로 어떠한 상황의 실내 디자인과도 자연스런 조화를 이루며 설치가 용이하고 유지보수가 간편하다.

2) 기  능

- 뛰어난 음성 명료도

- 슬림한 디자인

- 와이드 수평 분산

- 수직 빔 스티어링 (DDC 기술)

- 32비트 부동 소수점 DSP

- 수직 빔 제어

- 듀얼 라인 입력 지원

- 8밴드 파라 메트릭 EQ

- 8개의 사용자 정의 가능

- 암호로 보호 된 사전 설정

- 업그레이드 가능한 펌웨어

3) 사  양

- System type : 4“ Active Beam Steering Powered Loudspeaker Array

- Frequency Response (±3dB) (4”loudspeaker) : 230Hz ~ 10kHz

- Frequency Response (±3dB) (Complete array) : 130Hz ~ 10kHz

- Coverage : 130° (Horizontal),
opening angle 6 to 14°
elevation (aiming) angle -16 to 16°
focus distance 5 to 100m (Vertical)

- Power rating : 16 x 40W cont. (4 ohm)

- Max Peak SPL : 95dB

- Impedance : 6K8 ohms

- DSP module Type : floating point 900 MFLOPS 32 bits

- DSP module Sample rate : 48.8 kHz

- Transducers : 17 x 4” full range

- Connectors : pitch cage clamp

- Dimension (H x W x D)mm : 4350 x 134 x 92

- Weight : 37kg