HDMI OUTPUT BOARD (DGX-O-HDMI)

1) 용  도

본 기기는 전용 비디오 스위처에 장착하는 HDMI 출력 보드이며, 4개의 HDMI 포트가 오디오, 비디오 신호 전송을 지원한다.

2) 기  능

- InstaGate Pro® HDCP 인증키 기술

- 핫스왑 기능

- 3D 비디오 지원

- 서라운드 오디오 지원

3) 사  양

GENERAL

- Recommended Accessories: CBL-HDMI-FL HDMI High Speed Flat Cable (FG10-2180-16)

HDMI w/HDCP

- Compatible Formats: HDMI, HDCP, DVI

- Signal Type Support: HDMI, DVI-D (Single Link With HDMI Cable Adapter

- Video Data Rate (Max):

4.95 Gbps / 6.75 Gbps

6.75 Gbps supported when the HDMI Output Scaler or DXLink Rx Scaler is in Bypass mode and format is 1080p60 or less

- Video Pixel Clock (Max):

165 MHz / 225 MHz

225 MHz supported when the HDMI Output Scaler or DXLink Rx Scaler is in Bypass mode and format is 1080p60 or less

- Progressive Resolution Support:

480p up to 1920x1200 @ 60 Hz

If input is interlaced, all scaled outputs will deinterlace video to a progressive resolution format. If in scaler Bypass mode interlaced input will pass through unaltered

- Output Re-clocking: Yes

- Output Scaling: SmartScale, or optional manual configuration, or optional bypass

- SmartScale Output Resolution Support:

All resolutions between 480p and 1920 x 1200 @ 60 Hz via automatic SmartScale query of the display's declared EDID Detailed Timing Definition.

- Deep Color Support:

24-bit, 30-bit, 36-bit

30-bit and 36-bit supported when the HDMI Output Scaler or DXLink Rx Scaler is in Bypass mode and format is 1080p60 or less

- Color Space Support:

RGB 4:4:4;

YCbCr 4:4:4 and 4:2:2

Input signal support for YCbCr 4:4:4 and 4:2:2, output color-space is converted to RGB 4:4:4

- 3D Format Support:

Yes (HDMI Primary Formats)

Frame Packing 1080p up to 24 Hz

Frame Packing 720p up to 50/60 Hz

Frame Packing 1080i up to 50/60 Hz

Top-Bottom 1080p up to 24 Hz

Top-Bottom 720p up to 50/60 Hz

Side-by-Side Half 1080i up to 50/60 Hz

3D supported when the HDMI Output Scaler or DXLink RX Scaler is in Bypass mode and format is 1080p60 or less

- Audio Format Support:

Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS, 2 CH through 8 CH L-PCM

Dolby Digital and DTS support up to 48 kHz, 5.1 channels

- Audio Resolution: 16 bit to 24 bit

- Audio Sample Rate: 32 kHz, 44.1 kHz, 48 kHz, 96 kHz, 192kHz

- Local Audio Support: Yes, Insertion and/or Extraction of 2 CH L-PCM selectable by channel

- HDCP Support: Yes, full matrix HDCP support (includes any input to any or all outputs)

Key Management System

- AMX HDCP InstaGate Pro™ Technology:

Key support up to 16 devices per output, independent of source device

- CEC Support: None

- Output Voltage (Nominal): 1.0 Vpp Differential

- Output Rise Time / Fall Time:

100 ps min - 200 ps max (20% - 80%)

0.16 UI min - 0.33 UI max (@ 1.65 Gbps, 20% - 80%)

Output +5V DDC Pin: 50mA max per output port

- Connectors:

4 HDMI Type A Female Ports

HDMI Output Board Propagation Delay: 24 ms for progressive, 48 ms for interlace, 5 us when in Bypass mode

HDMI Audio Synchronization: Progressive and Interlace Video Formats @ 60 Hz frame rate: Audio is actively delayed to match video within 8ms leading or lagging