MULTIMODE FIBER I/O BOARD, SIMPLEX (EPICADGX288-VIO-MMF-S)

1) 용  도

본 기기는 전용 모듈식 광 매트릭스 스위쳐에 장착하여 사용하는 카드타입 모듈이며 개별 보드는 16 연결을 지원하며 각각의 연결이 입/출력 기능을 제공하는 16x16 매트릭스 설정이 제공되며 오디오를 포함한 선명한 고해상도 무압축 비디오가 내장 스케일러를 통해 자동으로 디스플레이에 맞게 스케일링 해주는 기능을 구현한다.

2) 기  능

- 멀티모드 광케이블 대응

- 16x16 매트릭스 설정

- 개별 포트가 입/출력 기능에 대응

- 내장 스케일러가 디스플레이 최적 해상도에 맞게 스케일링

3) 사  양

- Signal Type Support:

DXLink Multi-Mode Fiber, Simplex

(Connectivity between TX and Input Connection and Output Connection and RX requires matching model types, multimode to multimode or single mode to single mode. The backplane architecture of the Epica DGX 288 allows for single mode inputs to be routed to multimode outputs and vice versa)

- Compatible AMX Products:

Must be used in conjunction with an Epica 288 Matrix Switcher Enclosure and a DXLink Simplex Multimode Fiber Transmitter and/or Reciever including DXF-TX-MMS (FG1010-363) and DXF-RX-MMS (FG1010-563)

- Compatible Formats: HDMI Video / Audio over fiber

- Regulatory Compliance: See Epica 288 Matrix Switcher Enclosure for regulatory compliance

- Safety Certifications: Class 1 Eye Safe per requirements of IEC 60825-1 / CDRH

DXLINK FIBER

- Transport Layer Throughput: 10.3125 Gbps

- Video Data Rate (max.): 4.95 Gbps

- Video Pixel Clock (max.): 165 MHz

- Progressive Resolution Support: 480p up to 1920x1200,60 Hz

- Interlaced Resolution Support: 480i, 576i, 1080i

- 2K Resolution Support:

2048x1024,47Hz; 2048x1080,60Hz; 2048x1152,60Hz; 2048x1536,24Hz

2K formats are only compatible with DVI, HDMI, and DXLink Fiber Input/Output Boards and require the output or RX Scaler to be set in Bypass mode

- Deep Color Support: 24-bit

- Color Space Support:

RGB 4:4:4

YCbCr 4:4:4 and 4:2:2 (Input signal support is for YCbCr 4:4:4 and 4:2:2; output color-space is converted to RGB 4:4:4.)

- 3D Format Support:

Frame Packing 1080p up to 24 Hz

Frame Packing 720p up to 50/60 Hz

Frame Packing 1080i up to 50/60 Hz

Top-Bottom 1080p up to 24 Hz

Top-Bottom 720p up to 50/60 Hz

Side-by-Side Half 1080i up to 50/60 Hz

The scaler on the corresponding DXLink Fiber RX must be set to Bypass mode.

- Audio Format Support: Dolby TrueHD, Dolby Digital, DTS-HD Master Audio, DTS

2 CH through 8 CH L-PCM

Dolby Digital and DTS support up to 48 kHz, 5.1 channels

- Audio Resolution: 16 bit to 24 bit

- Audio Sample Rate: 32 kHz, 44.1 kHz, 48 kHz, 96 kHz, 192 kHz

HDCP Support: Full matrix HDCP support (includes any input to any or all outputs)

- Key Management System:

AMX HDCP InstaGate Pro® Technology

Key support up to 16 destinations per output/receiver, independent of source device

- CEC Support: None

- Connectors:

16 LC Simplex Fiber ports (with an input and an output connector on each) conforming to ANSI TIA/EIA 604-10 (FOCIS 10A)

Fiber Cable Types and Supported Length: OM3 50/125 mm @ 984 ft. (300 m)

- Optical Wavelength: 850 nm

- Multimode Optical Budget: 6.8 dB (typical) between DXLink Fiber transceivers

- Optical Modulation Amplitude (OMA): -4.3 dBm (min.)

- Optical Modulation Amplitude (OMA) Sensitivity: -11.1 dBm (typical)

- Multimode Optical Transceiver Mean Output Power: -1 dBm (average power)

- DXLink Fiber Input Port Propagation Delay: 5 ms

- DXLink Fiber Output Port Propagation Delay: 5 ms