PROFESSIONAL WIRELESS MICROPHONE SYSTEM (WMS420 PRESENTER SET)

1) 용  도

본 기기는 무선 마이크 시스템으로서, 최대 16채널을 같은 주파수 대역에서 운영할 수 있으며 파일럿톤이 지속적으로 뮤트 스위치의 위치 및 건전지 잔량을 수신기로 전송함으로서 소규모 클럽, 예배당, 회의실, 기악 및 성악 공연에 사용하기에 적합하다. 또한 시스템 시작시 일어날 수 있는 사고를 예방할 수 있으며 시스템 상태를 쉽게 모니터링 할 수 있도록 오디오 클리핑 및 RF 신호 LED를 제공한다.

2) 기  능

- 최대 16채널 지원

- 파일럿톤 지원

- 오디오 클리핑 및 RF 신호 LED 제공

3) 사  양

- package includes : 1 x Bodypack transmitter PT420

: 1 x Stationary receiver SR420

: 1 x Head-worn microphone C555 L

: 1 x Windscreen W444

: 2 x Receiver antennas

: 1 x AC adapter

: 1 x AA size battery

- Model : SR420

- Frequency bands : A = 530,025 – 559,000 MHz

U1 = 606,100 – 613,900 MHz

U2 = 614,100 – 629,900 MHz

B1 = 748,100 – 751,900 MHz

B2 = 774,100 – 777,900 MHz

M = 826,300 – 831,000 MHz

D = 863,100 – 864,900 MHz

K = 925,100 – 931,850 MHz

- Diversity system : Antenna switching

- RF output : 10, 20 or 50 mW (depending on frequency band)

- Audio bandwidth : 40 – 20 000 Hz (+/- 3dB)

- Tuning range : Up to 30 MHz (depending on frequency band)

- Max. channels : Up to eight compatible channels within one frequency band

- RF radiation : 50 mW max. (ERP)

- Frequency selection : Fixed frequencies

- Modulation : FM

- Radio range (Line of sight) : 30 meter

- Rack size : ½ Racksize (19”)

- Dimensions : 150 x 44 x 200 mm

- Model : PT420

- Type : Three pin mini XLR connector (female)

- Maximum audio level : 12dB

- Rated Impedance : 1 Ohms

- Audio bandwidth : 40 – 20 000 Hz (+/- 3dB)

- Signal to noise : 105 dB-A

- THD at 1kHz : 0.8%

- Transmitter synchronization : Manual

- Battery type : AA battery

- Operating time : Up to eight hours with one AA battery

- Dimensions : 60 x 75,5 x 30 mm

- Weight : 214g