REFERENCE WIRELESS STATIONARY RECEIVER (SR420)

1) 용  도

본 기기는 아날로그 무선 수신기로서, 사전 설정을 통해 최대 8개의 채널에 동시 사용이 가능하다. 소규모 클럽, 예배당, 회의실, 기악 및 성악 공연에 사용하기에 적합하며 시스템 상태를 쉽게 모니터링 할 수 있도록 오디오 클리핑 및 RF 신호 LED를 제공한다. 또한 XLR 및 1/4 "잭 커넥터를 제공하며 스위치 모드 전원 공급 장치 키트가 제공된다.

2) 기  능

- 착탈식 수신기 안테나

- 최대 30MHz 선택 대역폭

- 최대 8개의 채널 동시 사용 가능

- 밸런스 XLR 및 언밸런스 1/4 "잭 출력

- 수신기의 오디오 클립 및 RF 제어 LED 제공

- 가변 스퀠 치 레벨 제공

3) 사  양

- Frequency bands : A = 530,025 – 559,000 MHz

U1 = 606,100 – 613,900 MHz

U2 = 614,100 – 629,900 MHz

B1 = 748,100 – 751,900 MHz

B2 = 774,100 – 777,900 MHz

M = 826,300 – 831,000 MHz

D = 863,100 – 864,900 MHz

K = 925,100 – 931,850 MHz

- Diversity system : Antenna switching

- RF output : 10, 20 or 50 mW (depending on frequency band)

- Audio bandwidth : 40 – 20 000 Hz (+/- 3dB)

- Tuning range : Up to 30 MHz (depending on frequency band)

- Max. channels : Up to eight compatible channels within one frequency band

- RF radiation : 50 mW max. (ERP)

- Frequency selection : Fixed frequencies

- Modulation : FM

- Radio range (Line of sight) : 30 meter

- Rack size : ½ Racksize (19”)

- Dimensions : 150 x 44 x 200 mm