MID-HIGH LOUDSPEAKER

1) 용  도

본 기기는 매우 높은 출력의 듀얼 8“ 미드-하이 스피커로서 최고의 음질이 필요한 체육관, 운동장 등 사용이 가능하다. 최신 프리시전 디렉티비티(정확한 지향성) 기술이 탑재 되어 있으며, 낮은 전력 사용량으로 지속적으로 높은 음압을 유지 할 수 있다. 또한 상황에 따라서 WRC, WRX 마감옵션을 통하여 실외 사용이 가능하다.

2) 기  능

- 스피커 전면 치수는 대칭되어 40˚x30˚ 커버리지를 수직 또는 수평 방향 중 선택하여 사용

- IFS™ 혼선 방지 기능 내장

- 듀얼 8인치 혼-로드 콘으로 고출력의 스피커

- 코액시얼(동축) 중고역대 모듈 설계

- 프리시전 디렉티비티(정확한 지향성) 기술 적용

3) 사  양

- Frequency Range (+/-10 dB) : 200 Hz to 19.5 kHz

- Frequency Response (+/-3 dB) : 230 Hz - 18.5 kHz

- Coverage Pattern : 40˚ x 30˚

- Directivity Index : 16 dB

- System Sensitivity (1W @ 1m) : Passive Mid-High: 110 dB SPL

- Maximum Peak SPL : MHF - 142 dB Peak Passive Mode

- System Power Rating (IEC) : MHF - 400 W (1600 W Peak)

- Crossover Frequencies : 1.3 kHz

- Nominal Impedance : 4 Ohms Passive

- MF Driver : 2 x midrange driver with 8“ diameter Differential Drive® dual 3” voice coil

- HF Driver : 2 x 1.5“ exit compression driver, 3“ voice coil

- WRC/WRX Version Environmental Specifications : IP55

- Dimensions (H x W x D) : 991 x 991 x 1145.8 mm

- Net Weight : 111.4 kg